The phase retrieval program generates two outputs: the amplitude and phase retrieved from the time domain, and another from the frequency domain. Toptica’s phase retrieval gives me the same pulse when setting the field from either domain, but Henry’s code does not do that which seems odd to me.

Chart, histogram

Description automatically generated